{"text_format":"3","workbook":"xls","n_sheets":1,"sheets":["Sheet1"],"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Sheet1","index":0,"n_rows":14,"n_cols":6,"rows_kept":14,"merged":[[0,0,0,5],[13,1,13,5]],"flags":["formulas_cached_only"]}
["人民医院监控及报警"]
["序号","名称","参数要求","型号","单位","数量"]
[1,"半球","1.主码流支持2560x1440@25fps，子码流支持1280x720@25fps，第三码流支持1280x720。\n2.最低照度彩色0.005lx，黑白0.0005lx。\n3.内置GPU芯片，麦克风，扬声器。\n4.支持白光补光、红外补光，在开启白光灯进行补光时，可输出彩色视频图像。\n5.同一静止场景相同图像质量下，设备H.265、SmartH.265编码方式时，开启智能编码功能和不开启智能编码相比，码率节约80%。\n6.支持智能报警防干扰功能，智能分析行为类型为区域入侵、越界侦测、进入区域、离开区域时，报警检测目标设置为人体和/或车辆时，光线明暗变化，篮球滚动，狗行走，树摇晃，不触发报警。\n7.支持声音报警功能，报警声音类型不低于12种，并支持导入自定义语音，报警音量及重复次数可设置\n8.可对出现在监控画面中的两眼瞳距不小于26像素的人脸进行检测，并叠加目标提示框。\n9.支持像素显示功能，可通过IE浏览器显示预览画面中鼠标所选区域水平及垂直方向的像素数。\n10.支持快捷配置功能，可在预览画面页开启/关闭“快捷配置”页面，支持配置常用显示图像参数、OSD配置、音视频参数、智能资源分配等，并支持恢复默认操作。\n支持1路报警输入，1路报警输出，1路音频输入，1路音频输出，POE供电。",null,"台",78]
[2,"枪机","1.需支持三码流技术，可同时输出三路码流，主码流最高2688×1520@25fps，第三码流最大1280×720 @ 1fps，子码流1280×720@25fps。\n2.最低照度彩色0.0005lx，黑白0.0001lx。\n3.内置GPU芯片，麦克风，扬声器。\n4.支持白光补光、红外补光，在开启白光灯进行补光时，可输出彩色视频图像。\n5.同一静止场景相同图像质量下，设备在SmartH.265、H.265编码方式时，开启智能编码功能和不开启智能编码相比，码率节约80%。\n6.支持智能报警防干扰功能，智能分析行为类型为区域入侵、越界、进入区域、离开区域时，报警检测目标设置为人体或车辆时，光线明暗变化，篮球滚动，狗行走，树摇晃，不触发报警。\n7.支持声音报警功能，报警声音类型不低于12种，并支持导入自定义语音，报警音量和重复次数可设置。\n8.可对出现在监控场景内的两眼瞳距不小于19像素的人脸进行检验，并叠加目标提示框。\n9.可对检测区域内不低于10个行人进行检测、框选跟踪、评分和抓拍，可筛选和抓拍最佳人脸图片存储及上报中心，抓拍数量及图片大小可设，可上传全景照。\n10.支持像素显示功能，可通过IE浏览器显示监视画面中鼠标所选区域水平及垂直方向的像素数。\n11.支持快捷配置功能，可在预览画面页开启/关闭“快捷配置”页面，支持配置场景参数、常用图像参数、OSD配置、音视频参数、智能资源分配参数等，并支持恢复默认操作。\n12.支持1路报警输入，1路报警输出，1路音频输入，1路音频输出，POE供电。\n13.IP67防护等级，含安装支架。",null,"台",59]
[3,"交换机","1.配置：可用千兆POE电接口数量≥24，可用千兆光接口数量≥4\n2.支持独立的console管理串口\n3.交换容量：336Gbps/3.36Tbps\n4.转发性能：42Mpps/96Mpps\n5.支持最大32台设备混合堆叠\n7.产品符合CQC31-452422-2019认证规则要求,并提供相应的证书\n8.支持802.3ad规定的链路聚合功能(提供第三方检测报告)\n10.支持按端口划分VLAN，支持VLAN TRUNK(提供第三方检测报告)\n11.支持IPv4/IPv6 静态路由、RIP、OSPF\n12.支持广播风暴抑制\n13.支持IGMP Snooping\n14.支持基于源MAC地址、目的MAC地址的ACL(提供第三方检测报告)\n15.支持端口镜像\n16.可以为远程连接用户提供访问控制，拒绝未通过验证的连接\n17.支持通过TELNET对设备进行管理(提供第三方检测报告)\n19.每台配2块配套单模光模块\n",null,"台",18]
[4,"六类网线","六类 UTP 305米/箱",null,"箱",26]
[5,"硬盘","8T企业级存储专业硬盘，兼容宇视视频存储阵列（VX1848-V2）",null,"块",28]
[6,"2芯电线","2*1.0 屏蔽线 国标",null,"米",1800]
[7,"单防区扩展模块","配合福科斯FC-7448或FC-7400主机使用，不需外接供电，可直接接入总线（现有平台为福科斯）",null,"个",30]
[8,"紧急按钮","紧急报警，钥匙复位按钮开关",null,"个",35]
[9,"辅材","PVC管槽、扎带、电子标签、水晶头、跳线、跳纤、必要的熔纤等，不限于以上",null,"批",1]
[10,"一键式报警系统","东院一键式报警系统1年维保、包工包料",null,"项",1]
[11,"安装调试费",null,null,"项",1]
["合计"]